**Capital Giving Wall PCAM:**

Backer Panel – 11/16” clear P-95 acrylic w / 22-1/2 degree bevel mounted to ½” clear w/ white vinyl inner layer, satin edges

Cut Letters 1 – 2 1/2” x 1/2” Flat Cut Out Plate Letters, Bronze Alloy 220, Pin Mounted

Cut Letters 2 – 5 1/2” x 1” Fabricated Letters; Bronze Alloy 220, Pin Mounted

Confirm cap height of other giving levels